# I3C Basic Automation demo:

## Getting started:

1. Install the Logic 2 Automation API via pip as described in the [Getting Started documentation](https://saleae.github.io/logic2-automation/getting_started.html): 

        `pip install logic2-automation`

2. Run the Logic software with the Automation Server enabled:

- By enabling it directly in the software UI as explained [here](https://saleae.github.io/logic2-automation/getting_started.html#launching-logic2)
- Or from the command line as explained [here](https://saleae.github.io/logic2-automation/launching_logic2.html#launching-the-logic-2-software-and-starting-the-socket-interface) 

3. Configure in the **python script** the **Logic device ID**, the **License key**, (and the **Capture File Path** if you'll be loading an example capture").

4. Run the script.